# 4MP HD WDR IR Motorized Zoom Dome Network Camera

LS-PD24401M



## Key Features

* High quality image with 4MP, 1/3"CMOS sensor
* 4MP (2688\*1520)@ 30/25fps; 4MP (2560\*1440)@ 30/25fps; 3MP (2304\*1296) @30/25fps; 2MP (1920\*1080) @30/25fps;
* Ultra 265, H.265, H.264, MJPEG
* 2.8 ~ 12mm motorized zoom lens
* 120dB true WDR technology enables clear image in strong light scene
* Support 9:16 Corridor Mode
* Built-in Mic
* Smart IR, up to 40m IR distance
* Supports 256 G Micro SD card
* IP67 protection
* Support PoE power supply
* 3-Axis

## Specifications

|  |  |
| --- | --- |
|  | LS-PD24401M |
| Camera |
| Sensor | 1/3", 4.0 megapixel, progressive scan, CMOS |
| Lens | 2.8 ~ 12mm, AF automatic focusing and motorized zoom lens |
| DORI Distance | Lens (mm) | Detect (m) | Observe (m) | Recognize (m) | Identify (m) |
| 2.8 | 63.0 | 25.2 | 12.6 | 6.3 |
| 12 | 180 | 72 | 36 | 18 |
| Angle Of View (H) | 102.79°~ 30.86° |
| Angle Of View (V) | 54.50°~ 17.49° |
| Angle Of View (O) | 106.94°~35.49° |
| Adjustment Angle | Pan: 0° ~ 360° | Tilt: 0° ~ 90° | Rotate: 0° ~ 360° |
| Shutter | Auto/Manual, 1 ~ 1/100000s |
| Minimum Illumination | Support Easystar: Colour: 0.003Lux ( F1.6, AGC ON) 0Lux with IR |
| Day/Night | IR-cut filter with auto switch (ICR) |
| Digital Noise Reduction | 2D/3D DNR |
| S/N | >56dB |
| IR Range | Up to 40m IR range |
| Wavelength | 850nm |
| IR On/Off Control | Auto/Manual |
| Defog | Digital Defog |
| WDR | 120dB |
| Video |
| Video Compression | Ultra 265, H.265, H.264, MJPEG |
| H.264 Code Profile | Baseline profile, Main profile, High profile |
| Frame Rate | Main Stream: 4MP (2688\*1520), Max 30fps;4MP (2560\*1440), Max 30fps; 3MP (2304\*1296), Max 30fps; 1080P (1920\*1080), Max 30fps;Sub Stream: 720P (1280\*720), Max 30fps; D1 (720\*576), Max 30fps; 640\*360,Max 30fps; 2CIF(704\*288), Max 30fps; CIF(352\*288), Max 30fps; |
| Video Bit Rate | 128 Kbps~16 Mbps |
| 9:16 Corridor Mode | Supported |
| OSD | Up to 4 OSDs |
| Privacy Mask | Up to 4 areas |
| ROI | Up to 8 areas |
| Motion Detection | Up to 4 areas |
| Image |
| White Balance | Auto/Outdoor/Fine Tune/Sodium Lamp/Locked/Auto2 |
| Digital Noise Reduction | 2D/3D DNR |
| Smart IR | Support |
| Flip | Normal/Vertical/Horizontal/180°/90°Clockwise/90°Anti-clockwise |
| Dewarping | N/A |
| HLC | Supported |
| BLC | Supported |
| Audio |
| Audio Compression | G.711 |
| Suppression | Supported |
| Sampling Rate | 8KHZ |
| Storage |
| Edge Storage | Micro SD, up to 256GB |
| Network Storage | ANR, NAS(NFS) |
| Smart |
| Behavior Detection | Cross line, intrusion(based on human body detection) |
| motion detection, tampering alarm, audio detection |
| General Function | Watermark, IP address filtering, access policy, ARP protection, RTSP authentication, user authentication, HTTP authentication |
| Network |
| Protocols | IPv4, IGMP, ICMP, ARP, TCP, UDP, DHCP, RTP, RTSP, RTCP, RTMP, DNS, DDNS, NTP, FTP, UPnP, HTTP, HTTPS, SMTP, SSL, 802.1x, SNMP |
| Compatible Integration | ONVIF (Profile S, Profile G, Profile T) |
| Web Browser | Plug-in required live view: IE9+, Chrome 41 and below, Firefox 52 and below |
| Plug-in free live view: Chorme 57.0+, Firefox 58.0+, Edge 16+, Safari 11+ |
| Interface |
| Network | 10/100M Base-TX Ethernet |
| Built-in Mic | Supported |
| General |
| Power | DC 12V±25%, PoE (IEEE 802.3af) |
| Power consumption: Max 8.50W |
| Material | Metal |
| waterproof | IP67 |
| Working Environment | -30°C ~ 60°C (-22°F ~ 140°F), Humidity: ≤95% RH (non-condensing) |
| Strorage Environment | -30°C ~ 60°C (-22°F ~ 140°F), Humidity: ≤95% RH (non-condensing) |
| Product size/weight | Φ129 x 110mm/0.66kg |
| Packing size/weight | 155 x 155 x 140mm/0.86kg |

### Dimensions

